Arduino

## LoRa shield library

Arduino library for LoRa shield . This library concerns the LoRa Arduino shield that uses the SX1278 SEMTECH tranceiver. Three classes: SX1278 ; basic modem management. LORA ; simplified functions for LoRa modem REMOTEC ; simplified functions for using SX1278 as OOK transitter with HX2262 protocol Both LORA class and REMOTEC class use basic SX1278 functions. So, you can use SX1278 functions mixed with LORA or REMOTEC functions for better trim. SX1278 class is referenced by external name SX. Pin used by shield: D13 : SPI SCK D12 : SPI MISO D11 : SPI MOSI D10 (or D8) : SPI CS D5 (or D7) : SX1278 RESET (D6 or D9 or none) : Inp/Out pulses (D3 or none) : interrupt |  | #### Classes SX1278 LORA REMOTEC Datasheet sx1278 #### Examples LoRaTxEcho LoRaRxEcho RemPwr RemPwrScanner

Reference Home

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes